# K2Aley GAR-BOT 3D Print Queue

Copyright (c) 2026 K2Aley. GAR-BOT. All rights reserved.

| Priority | Qty | Part file/module | Material | Purpose |
| ---: | ---: | --- | --- | --- |
| 1 | 1 | `electronics_bay` | PETG/ASA | Seals RP5, relay HAT, Pico Voice header path, and wiring |
| 1 | 1 | `gasketed_lid` | PETG/ASA + gasket | Seals electronics bay |
| 1 | 1 | `cable_gland_panel` | PETG/ASA | Routes wires through glands |
| 1 | 4 | `ibt2_driver_cover` | PETG/ASA | Covers motor drivers |
| 1 | 1-2 | `buck_converter_cover` | PETG/ASA | Covers buck converters |
| 1 | 4 | `motor_splash_shield` | PETG/ASA | Protects motors |
| 1 | 1 | `frame_left_side_rail` | PETG/ASA | Left chassis rail with motor and deck mounting holes |
| 1 | 1 | `frame_right_side_rail` | PETG/ASA | Right chassis rail with motor and deck mounting holes |
| 1 | 1 | `frame_front_crossmember` | PETG/ASA | Front frame crossmember and bumper tie point |
| 1 | 1 | `frame_rear_crossmember` | PETG/ASA | Rear frame crossmember and tow/handle tie point |
| 1 | 1 | `frame_bottom_skid_plate` | PETG/ASA | Lower splash and skid plate |
| 1 | 1 | `frame_center_battery_tray` | PETG/ASA | Battery tray with strap slots and retaining lips |
| 1 | 1 | `frame_electronics_deck_plate` | PETG/ASA | Deck plate for sealed electronics bay mounting |
| 2 | 1 | `touchscreen_bezel` | PETG/ASA | Gasketed 7 inch touchscreen frame |
| 2 | 1 | `touchscreen_rain_hood` | PETG/ASA | Screen rain hood |
| 2 | 1 | `frame_touchscreen_upright_left` | PETG/ASA | Left support for 7 inch touchscreen frame |
| 2 | 1 | `frame_touchscreen_upright_right` | PETG/ASA | Right support for 7 inch touchscreen frame |
| 2 | 1 | `frame_touchscreen_top_bar` | PETG/ASA | Top tie bar for touchscreen uprights |
| 2 | 1 | `left_claw_base_mount` | PETG/ASA | Mounts left claw |
| 2 | 1 | `right_claw_base_mount` | PETG/ASA | Mounts right claw |
| 2 | 1 | `frame_claw_bridge` | PETG/ASA | Forward shoulder bridge for both claw pivots |
| 2 | 2 | `round_shoulder_mount` | PETG/ASA | Round claw pivots |
| 2 | 2 | `sealed_servo_pocket` | PETG/ASA | Servo protection |
| 2 | 2 | `wrist_servo_cradle` | PETG/ASA | Wrist servo support |
| 2 | 2 | `claw_palm` | PETG/ASA | Gripper palms |
| 2 | 4 | `claw_gripper_finger` | PETG/ASA | Two fingers per claw |
| 2 | 4-8 | `claw_link_bar` | PETG/ASA | Claw link bars |
| 2 | 2 | `claw_gear_guard` | PETG/ASA | Gear guards |
| 2 | 2 | `forearm_wire_cover` | PETG/ASA | Covers claw wiring |
| 2 | 2 | `claw_controller_cover` | PETG/ASA | Covers claw control boards |
| 3 | 12-20 | `drip_loop_cable_clip` | PETG | Wire drip loops |
| 3 | 1 | `k2aley_lid_badge` | PETG/ASA | Raised logo |
| 3 | 2 | `k2aley_side_badge` | PETG/ASA | Side branding |
| 3 | 1 | `water_warning_badge` | PETG/ASA | Wet-use warning |
| 3 | 1 | `remote_zero2w_pico_voice_case_front` | PETG/ASA | Front shell for RP Zero 2 W + Pico Voice transmitter |
| 3 | 1 | `remote_zero2w_pico_voice_case_back` | PETG/ASA | Rear shell for transmitter battery and boards |
| 3 | 1 | `remote_lora_antenna_bulkhead` | PETG/ASA | Remote LoRa antenna mount |
